Anexa 10.a.
Certificatului CEMT de conformitate cu cerințele tehnice și de siguranță pentru autovehicule
 „EURO V/ 5 sigur”, „EEV sigur”, „EURO VI/ 6 sigur” și „ZEV”
cu masa maximă autorizată cuprinsă între 3,5 și 6 tone”, cf Ghidul CEMT 2027
(incluzând cazul specific al autovehiculele peste 6 tone 1).
varianta în limba engleză 
Hârtie verde deschis, imprimată față/verso
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Certificate No:

ECMT Certificate of Compliance with Technical and Safety Requirements for a Motor
Vehicle (Lorry) with TPLW above 3.5 and not exceeding 6 Tonnes
Q "EURO V5 safe” Q "EEV safe” Q "EURO VI/6 safe”" 0 “ZEV»
[Vehicle Type and Make:
Vehicle Identification Number (VIN):
Engine Type / Number:
The?

~  Competent validation Services in the country of registration.>

- Vehicle Manufacturer, or the authorised Representative of the Manufacturer in the country of
registration, or

- A combination of the competent validation Services in the country of registration and the
‘vehicle Manufacturer. or the authorised Representative of the Manufacturer in the country of
registration. when all the equipment is not fitted by the vehicle Manufacturer.*

[Name(s) and stamp(s) of the Company and/or the Administration]

hereby confirms that the said vehicle is in compliance with the provisions of respective UN Regulations and/or EU
regulatory acts, as listed below, and confirms tht the particulars entered overleaf are correct.

ENGINE POWER

O O Measurements according to: UN Regulation No 85.00 or as subsequently amended: or to Directive
80/1269/EEC. as amended by Directive 1999/99/EC or as subsequently amended.
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REQUIREMENTS FOR NOISE AND EXHAUST EMISSIONS

a

a

a

a

Delete

‘Noise measured according to: UN Regulation No 51.02 or as subsequently amended: or to Regulation (EU)
No 54012014 or as subsequently amended.

EURO V/5: Type-approval of engines with respect to emissions according to UN Regulation No 49.04.
fow B2 or as subsequently amended; o to Directive 2005/55/EC as amended by Directive 2005/78/EC.
fow B2 or as subsequently amended % or type-approval of vehicle according to UN Regulation No 83.06;
or to Regulation (EC) No. 715/2007 as amended by Regulation (EC) No 692/2008. or as subsequently
amended &

EEV: Type-approval of engines with respect to emissions according to UN Regulation No 49.04, row C
or as subsequently amended: or to Directive 2005/55/EC as amended by Directive 2005/78/EC, row C or
as subsequently amended ”

EURO VI/6: Type-approval of engines with respect to emissions according to UN Regulation No 49.06;
or to Regulation (EC) No 595/2009 as amended by Commission Regulation (EU) No 582/2011 and
Commission Regulation (EU) No 642012 or as subsequently amended;® or type-approval of vehicle
according to UN Regulation No. 83.07 or Regulation (EC) No. 715/2007 as amended by Regulation (EC)
No. 692/2008, or as subsequently amended.”

‘Lories above 6 tomnes type approved according to light duty vebicle emissions regulations or equipped with pefrol engines are included.

‘mentions

inappropriate
For the countries where the Representativs of the mamfacturers ae not authorised.
In this case, the first Signatory fllinthe column on the e, the second Signatory il in the column on he right.
Character B2 or D, E. F or G, in the approval mumber
Character A to M in the approval mumber.
Character C or H, L J orK in the approval mumber
Character A, B, C, D or E n the approval mumber.
Character N to ZZ: A or a subsequently amended. n the approval mumber
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O O ZEV: Type-approval of engines with respect to emissions according to UN Regulation No 49.06: or to

Regulation (EU) 2018/858 as amended by Regulation (EU) No 2019/2144 or as subsequently amended.

SAFETY REQUIREMENTS
The motor vehicle is fitted with the following devices:

Rear underrun protective devices™ according to UN Regulation No 58.02 o as subsequently amended: or
to Regulation (EU) 2019/2144 or as subsequently amended.

Lateral protection™® according to UN Regulation No 73.00 or as subsequently amended: or to Regulation
(EU) 2019/2144 or as subsequently amended.

Devices for Indirect vision according to UN Regulation No 46.03 or as subsequently amended: or to
Regulation (EU) 2019/2144 or as subsequently amended.

Installation of lighting and light-signalling devices according to UN Regulation No48.03 or as
subsequently amended: or to Regulation (EU) 2019/2144 or as subsequently amended

EURO V/5 or EEV: Digital tachograph according to the UN AETR Agreement or its amendments, or to
Council Regulation (EEC) No 3821/85 as amended by Regulation (EC) No. 2135/98 or as subsequently
amended. as well as by Commission Regulation (EU) No. 1266/2009 or as subsequently amended: or

EURO V/5 or EEV: Smart tachograph according to Regulation (EU) No. 165/2014 implemented by
Commission Implementing Regulation (EU) 2016/799 and amended by Commission Implementing
Regulation (EU) 2018/502 or as subsequently amended.

EURO VU6 or ZEV: Digital tachograph according to the UN AETR Agreement or its amendments, or
to Council Regulation (EEC) No 3821/85 as amended by Regulation (EC) No. 2135/98 or as subsequently
amended. as well as by Commission Regulation (EU) No. 1266/2009 or as subsequently amended: or
EURO VU6 or ZEV: Smart tachograph according to Regulation (EU) No 165/2014 implemented by
Commission Implementing Regulation (EU) 2016/799 and amended by Commission Implementing
Regulation (EU) 2018/502 or as subsequently amended.

Speed limitation devices according to UN Regulation No 89.00 or as subsequently amended: or to
Regulation (EU) 2019/2144 or as subsequently amended.

Braking, including anti-lock braking systems according to UN Regulation No 13.10 or as subsequently
amended; or to Regulation (EU) 2019/2144 or as subsequently amended.

Steering equipment according to UN Regulation No 79.01 or as subsequently amended: or to Regulation
(EU) 2019/2144 or as subsequently amended.
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10. Sems-raier tractor excepted.
11, Certificate may be filled in, stamped and signed manually or electronically.




