

Anexa 9 a.  
Modelul certificat CEMT de conformitate cu cerințele tehnice și de siguranță pentru (auto)vehicule, cf Ghid CEMT 2027
„EURO V sigur”, „EEV sigur”, „EURO VI sigur” sau „ZEV” 
- varianta în limba engleză
Hârtie verde deschis, imprimată față / verso
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Certificate No:

ECMT Certificate of Compliance with Technical and Safety Requirements for a Motor Vehicle
Q0 "EURO V safe" Q "EEV safe" Q "EURO VI safe" Q"ZEV"

Vehicle Type and Make:
Vehicle Identification Number (VIN):
Engine Type / Number:

Thel
~  Competent validation Services in the country of registration,”
- Vehicle Manufacturer, or the authorised Representative of the Manufacturer ia the country of
registration. or
- Acombination of the competent validation Services in the country of registration and the vehicle
Manufacturer, or the authorised Representative of the Mamufacturer in the country of regisiration.
when all the equipment is not fitted by the vehicle Manufacturer.®

[Name(s) and stamp(s) of the Company and/or the Administration]
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hereby confirms that the said vehicle is in compliance with the provisions of respective UN Regulations and/or EU
regulatory acts, as lsted below, and confirms that the particulars entered overleaf are correct.

ENGINE POWER

o a

Measuzements according to: UN Regulation No 85.00 or as subsequently amended: or Directive 80/1269/EEC.
as amended by Directive 1999/99/EC or as subsequently amended.

REQUIREMENTS FOR NOISE AND EXHAUST EMISSIONS

o a
o a
o a
o a

Noise measured according to: UN Regulation No 51.02 or as subsequently amended: or Regulation (EU)
No 540/2014 or as subsequently amended.

EURO V: Type-approval of engines with respect to emissions according to UN Regulation No 49.04, row B2
or as subsequently amended: or to Directive 2005/55/EC as amended by Directive 2005/78/EC. row B2 or as
subsequently amended *

EEV: Type-approval of engines with respect to emissions according to UN Regulation No 49.04, row C or as
subsequently amended: or to Directive 2005/S5/EC as amended by Directive 2005/78/EC. row C or as
subsequently amended

EURO VI: Type-approval of engines with respect to emissions according to UN Regulation No 49.06; or to
Regulation (EC) No 595/2009 as amended by Commission Regulation (EU) No 582/2011 or as subsequently
amended ©

O O ZEV: Type-approval of engines with respect to emissions according to UN Regulation No 49.06: or to
Regulation (EU) 2018/858 as amended by Regulation (EU) No 2019/2144 or as subsequently amended.
Delete inappropriate mentions.

For the counfries where the Representatives of the manufacturers are not authorised
In this case, the firt Signatory fllin the column on the Ief.the second Signatory fllsinthe column on the right
Character B2, or E or G, in the approval number

Character C,or L, arK. inthe approval mumber.

Character A, B, C, D, or E, in the approval mumber.
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SAFETY REQUIREMENTS
The motor vehicle is fitted with the following devices:

Q O Rear underrun protective devices” according to UN Regulation No 58.02 or as subsequently amended: or to
Regulation (EU) 2019/2144 or as subsequently amended.

QO Q Lateral protection” according to UN Regulation No 73.00 or as subsequently amended:, or to Regulation (EU)
2019/2144 or as subsequently amended.

Q QO Devices for Indirect vision according to UN Regulation No 46.03 or as subsequently amended: or to Regulation
(EU) 2019/2144 or as subsequently amended.

Q Q Installation of lighting and light-signalling devices according to UN Regulation No 48.03 or as subsequently
amended: or to Regulation (EU) 2019/2144 or as subsequently amended.

O O EUROV orEEV: Digital tachograph according to the UN AETR Agreement o its amendments, or to Council
Regulation (EEC) No. 3821/85 as amended by Regulation (EC) No. 2135/98 or as subsequently amended. as
well as by Commission Regulation (EU) No. 1266/2009 or as subsequently amended. or

O O EUROV or EEV: Smart tachograph according to Regulation (EU) No. 1652014 implemented by
Commission Implementing Regulation (EU) 2016/799 and amended by Commission Implementing Regulation
(EU) 2018/502 or as subsequently amended.

O O EURO VIor ZEV: Digital tachograph according to the UN AETR Agreement or its amendments. or to Council
Regulation (EEC) No. 3821/85 as amended by Regulation (EC) No. 2135/98 or as subsequently amended. as
‘well as by Commission Regulation (EU) No. 1266/2009 or as subsequently amended. or

O O EUROVI or ZEV: Smart tachograph according to Regulation (EU) No 1652014 implemented by
Commission Implementing Regulation (EU) 2016/799 and amended by Commission Implementing Regulation
(EU) 2018/502 or as subsequently amended.

Q QO Speed limitation devices according to UN Regulation No 89.00 or as subsequently amended: or to Regulation
(EU) 2019/2144 or as subsequently amended.

Q O Rear marking plates (setroreflective) for heavy and long vehicles according to UN Regulation No 70.01 or as
subsequently amended

Q  Q Braking, including anti-lock braking and electronic stability control function according to UN Regulation
No 13.11 or as subsequently amended.

Q QO Steering equipment according to UN Regulation No 79.01 or as subsequently amended: or to Regulation (EU)
2019/2144 or as subsequently amended.

Place Date ‘Signature(s) and stamp(s)”
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7. Semi-raler ractor excepted

8. Or, conspicuity marking according to UN Regulation No.48.03 or as subsequently amended.
9 Certificate may be filled in stamped and sisned manually or electromically.




