Anexa 9.c. 
Modelul certificatului de Inspecție Tehnică pentru autovehicul/autotractor și semiremorcă/remorcă, cf Ghid CEMT 2027
varianta în limba engleză,
Hârtie albă, format A 4, imprimat pe o față
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Certificate No:

ECMT Certificate of Roadworthiness Test for Motor Vehicles and Trailers’

Registration Number:

Certificate of Compliance Number.

Vehicle Type and Make:>

Vehicle Identification Number (VIN):

Engine Type / Number:>

The
[Name and adress of the Company or Authority]

Body or Establishment designated and directly supervised by the State of Registration for the purpose of
UN Agreement of 1997, or of the UN Consolidated Resolution RE.1 (TRANS/SC.1/294/Rev.5) as
amended in 2001 (TRANS/WP.1/2001/25) or as subsequently amended, or of Directive 2014/45/EU or as
subsequently amended,

hereby confirms that the said vehicle is in compliance with the provisions of the texts above, including at
least the following items to be compulsory checked:

Braking systems (including anti-lock braking systems, compatible with the trailer and vice-versa)
Steering wheel’ and steering devices

Visibility

Lamps, reflectors and electrical equipment

Axles, wheels, tyres and suspension (including minimum tread depth of tyres)
Chassts and chassis attachments (ncluding rear and lateral protective devices)
Other equipment, including:

a ‘Warning triangle’

Q0 Tachograph (presence of and integrity of seals)®

a Speed limitation device®

Exhaust emissions™* 3
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Place Date Signature and stamp®

Note:  Next roadworthiness test required by -

Semi.traiers inchuded.
Trailr type. iftrailer.

Not applicable to traier

Including, according to UN regulation No 24.03 and UN regulation No 49.03 or as subsequently amended
Not applicable to ZEVs.

Certificate may be fille in, stamped and signed manally or electronicaly.

The Certificate is valid 12 months after the date of the test, and at the latest before the end of this same month.




